## ST-713-187B

## Saturn Cartdev SIMM expansion buffer board

| Description: SIMM buffer board will hold 8 or 16 megabytes of RAM. Board is installed between the Cartdev and Saturn cartridge slot. Allows the programmer to use additional memory space when program files are too large for Saturn memory. If more space is needed, VCD or Mirage is the next step. Uses 72 pin SIMM (not included).

Features:

- Works in-line with Cartdev development system
- Uses standard 72 pin SIMM (not included)
- 8 or 16 megabyte capacity
- Buffer board with 2 slots for 72pin memory

Parts included:

SIMM expansion buffer board